1 Program 3T toafni

1.1 Purpose

Get information about current imaging sequence from the MCW Bruker 3T/60 scanner, format it for AFNI, and send it to AFNI. The output is written to stdout (AFNI will pipe it into itself).

1.2 Usage

3T toafni [-dummy]

1.3 Options

-dummy If the -dummy option is used, then the data from the scanner will be read from stdin instead of from the scanner console computer.