1 Program 3dproject

1.1 Purpose

Program 3dproject projects datasets along the three orthogonal directions to produce (up to) three 2D image files. Its options are to

ffl Project using the voxel sum, or using the voxel max along each ray.

ffl Edit out negative values.

ffl Project over the entire thickness of the dataset, or over any subrange (e.g., it is possible to get left hemisphere and right hemisphere projections separately).

Program 3dproject does not produce a brain outline or Talairach grid to provide any reference for projected images.

The output image files are by default in the internal AFNI format. This may not be useful for you, so you can either write them as ‘normal sized’ files with the -nsize option, or use program nsize (supplied with AFNI ) to convert them later.

1.2 Usage

The command line format for program 3dproject is as follows:

3dproject [editing options][-sumj-maxj-amaxj-smax] [-output root] [-nsize] [-mirror] [-RL fall j x1 x2g] [-AP fall j y1 y2g] [-IS fall j z1 z2g] [-ALL] dataset

The options are explained below.

1.3 Options

-sum Add the dataset voxels along the projection direction.

-max Take the maximum of the voxels along the projection direction.

-amax Take the absolute maximum of the voxels along the projection direction.

-smax Take the signed maximum of the voxels along the projection direction.

For example:

Option Voxel values Projected value -sum -7, 2, 4, 5 4 -max -7, 2, 4, 5 5 -amax -7, 2, 4, 5 7 -smax -7, 2, 4, 5 -7

Note: The default is -sum.

-nsize Scale the output images up to ’normal’ sizes (e.g., 64x64, 128x128, or 256x256). This option only applies to byte or short datasets.

-mirror The radiologists’ and AFNI convention is to display axial and coronal images with the subject’s left on the right of the image; the use of this option will mirror the axial and coronal projections so that left is left and right is right.

-output root Output projections will be named root.sag, root.cor, and root.axi. The default root is ’proj’.

-RL all Project in the Right-to-Left direction along all the data (produces root.sag)

-RL x1 x2 Project in the Right-to-Left direction from x-coordinate x1 to x2 (mm) (negative x is Right, positive x is Left). Or, you may use something like -RL 10R 20L to project from x=-10 mm to x=+20 mm.

-AP all Project in the Anterior-to-Posterior direction along all the data (produces root.cor)

-AP y1 y2 Project in the Anterior-to-Posterior direction from y-coordinate y1 to y2 (mm) (negative y is Anterior, positive y is Posterior). Or, you may use something like -AP 10A 20P to project from y=-10 mm to y=+20 mm.

-IS all Project in the Inferior-to-Superior direction along all the data (produces root.axi)

-IS y1 y2 Project in the Inferior-to-Superior direction from z-coordinate z1 to z2 (mm) (negative z is Inferior, positive z is Superior). Or, you may use something like -IS 10I 20S to project from z=-10 mm to z=+20 mm.

-ALL ==¿ Equivalent to ’-RL all -AP all -IS all’.

1.4 Notes

ffl A projection direction will not be used if the bounds aren’t given for that direction;

thus, at least one of -RL, -AP, or -IS must be used, or nothing will be computed!

ffl In the directions transverse to the projection direction, all the data is used; that is, ’-RL -5 5’ will produce a full sagittal image summed over a 10 mm slice, irrespective of the -IS or -AP extents.

ffl The [editing options] are the same as in 3dmerge. In particular, the ’-1thtoin’ option can be used to project the threshold data (if available).

1.5 Example

Example 1. The user wishes to project, over the entire thickness of the dataset, the AFNI 3D dataset anat+orig along the three orthogonal directions to produce three 2D image files. The command line is:

3dproject -ALL -output fred anat+orig The resulting AFNI 2D datasets are: fred.axi, fred.cor, and fred.sag.